**Packing list**

**Rotary Evaporator Model: R-1020CE**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **NO** | **Name** | **Unit** | **Quantity** | **Note** |
| 1 | User Manual | Pe | 1 |  |
| 2 | Main machine + Water bath | Set | 1 |  |
| 3 | Condenser pole | Pe | 1 |  |
| 4 | Condenser fixed clamp, support | Set | 1 |  |
| 5 | Cross clamp | Pe | 2 |  |
| 6 | Adjustment screw nut | Set | 1 |  |
| 7 | Condenser tray | Pe | 1 |  |
| 8 | Receiving flask tray | Set | 1 |  |
| 9 | Vacuum gauge, support, frame | Set | 1 |  |
| 10 | Main condenser | Pe | 1 |  |
| 11 | Auxiliary condenser | Pe | 1 |  |
| 12 | Condenser air suction nozzle | Set | 5 |  |
| 13 | 3-way flask | Pe | 1 |  |
| 14 | 40# Feeding valve | Set | 1 | Including 15# Valve |
| 15 | Evaporating flask 20L | Pe | 1 |  |
| 16 | Receiving flask 10L | Pe | 1 |  |
| 17 | 15# Discharge valve body | Pe | 1 | Including 15# Valve |
| 18 | Air release valve | Pe | 2 | Including 15# Valve |
| 19 | Glass rotation axis | Pe | 1 |  |
| 20 | Feeding tube F4 | Pe | 1 |  |
| 21 | Evaporating flask locknut, retaining ring, sealing kit | Set | 1 |  |
| 22 | Three flask locknut, retaining ring, F4 sealing ring | Set | 1 |  |
| 23 | Quick release flange, F4 sealing ring | Set | 7 |  |
| 24 | Alien wrench | Pe | 1 | S5 |
| 25 | Evaporating flask cap spanner | Pe | 1 |  |
| 26 | Stainless Steel alien screw | Pe | 4 | Мб X 8 2 pieces M6X12 2pieces |